|  |  |
| --- | --- |
| **English texts** | **Revised texts** |
| “Zowi workbech starting…” | “System start-up …” |
| Change switch to start process | Set to CALIBRATE position |
| Push to realize Cal. Horizontal | Press to set HORIZONTAL |
| Shutting down... | System shutting down…. |
| Place shoes in Horizontal box | Place shoes in Horizontal box |
| Calibrating Horiz. position | Calibration in progress... |
| Horizontal calib. failed. Retry | Process failed. Retry. |
| Horizontal done. Insert Vertical | Place shoes in Vertical box |
| Push to realize Cal. Vertical | Press to set VERTICAL |
| Place shoes in Vertical box | Place shoes in Vertical box |
| Calibrating Vertic. position | Calibration in progress... |
| Plug, Switch on, Put on and Push | Connect+ON ZOWI.Put shoes+press |
| Initializing communication | Checking connection... |
| Timeout. Check Zowi and push | Timeout. Check ZOWI+press |
| Connection fault. Check Zowi | Connection fault. Check ZOWI |
| Communication OK. Calibrating... | Communication OK. Calibrating... |
| CALIBRATION FAILED | CALIBRATION FAILED |
| Calibration OK. Writing EEPROM | Calibration OK. Writing EEPROM |
| Calibration OK. Loading Test Prg | Calibration OK. Loading Test Prg |
| Push for a new calibration | Press for a new calibration |