* **load all data:**

select \* from zowi.calibracion

* **load all data timestamp ordered by asc or desc:**

select \* from zowi.calibracion order by timestamp desc

select \* from zowi.calibracion order by timestamp asc

* **load all data serial number ordered by asc or desc:**

select \* from zowi.calibracion order by serial\_number desc

select \* from zowi.calibracion order by serial\_number asc

* **load ok calibrations:**

select \* from zowi.calibracion where state=1 AND serial\_number !=1

tip: serial\_number!= 1 for power on filtering

* **load nok calibrations:**

select \* from zowi.calibracion where state=0 AND serial\_number !=0

tip: serial\_number!= 0 for shutdown filtering

* **load nok calibrations with a specific joint error> xº:**

select \* from zowi.calibracion where (e\_left\_hip>= 1 OR e\_left\_hip<=-1) AND serial\_number!=1

* **load nok calibrations with a specific joint error between two values:**

select \* from zowi.calibracion where (e\_left\_hip between -1 AND 1) AND serial\_number !=1 AND serial\_number !=0

* **load power ons and shutdowns ordered in time:**

select \* from zowi.calibracion where (serial\_number=0 OR serial\_number=1) order by timestamp desc